|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| Model | | 60ft | I 100ft | I 150ft |
| BNC connector | Material | BNCM white rubber core, surface nickel-plated | | |
| Internal mode | PE | | |
| External mode | PVC(45P) yellow | | |
| Power connector | Male | DC5.5'2.1, black rubber core | | |
| Female | DC5.5'6.0, pin 2.1'18mm, white rubber core | | |
| External mode | PVC(45P) red | | |
| Video cable | Conductor material | Bare copper | | |
| Conductor wire gauge | HDPE(7/0.15)"1C+S(31/0.12)  CCA(copper clad aluminum ) | | |
| Jacket material | PVC | | |
| Jacket diameter | 2.6mm | | |
| Jacket color | Black | | |
| Power cable | Conductor material | Bare copper | | |
| Conductor wire gauge | Red(7/0.15)"1C+ PE(7/0.12)+250D nylonR1C | | |
| Jacket material | PVC | | |
| Jacket diameter | 2.6mm | | |
| Jacket color | Black | | |
| General | Length | 18.3m(60ft) | I 30.5m(100ft) | I 45.7m(150ft) |
| Working temperature | -40' — +80' | | |
| Storage temperature | -20' — +70' | | |
| Weight | 335g | 560g | 830g |
| Qty In Protective Box: | 48 In 1(with PE packaging) | 32 In 1(with PE packaging) | 24 In 1(with PE packaging) |
| Protective Box Dimension: | 400x330x200mm | | |
| Protective Box Weight(with accessories): | 16.5Kg | 18.5Kg | 20.5Kg |